{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"merged":[[0,0,0,7],[1,0,1,7],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[30,0,32,7]]}
["中国科学院广州生物医药与健康研究院                                                           L2栋202心理咨询室建设项目工程量清单"]
["工程名称:L2栋202心理咨询室建设项目"]
["序号","项目名称","项目特征描述","计量\n单位","工程量","综合单价","合价","备注"]
[]
[1,"乳胶漆（净味，无甲醛、环保）","1.基层类型:墙体\n2.腻子:刮腻子两遍\n3.油漆品种、刷漆遍数:乳胶漆(一底两面)","m2","180",null,null,"立邦：颜色由业主定"]
[2,"轻钢龙骨隔断","1.骨架、边框材料种类、规格:U75轻钢龙骨\n2.隔板材料品种、规格、颜色:10mm阻燃板+8mm厚硅酸钙板（双面），内填80厚玻璃棉板\n3.嵌缝、塞口材料品种:嵌缝腻子","m2","24.8",null,null,"泰山"]
[3,"成品高隔断配套木门（对开）","1.门类型:成品高隔断配套木门\n2.材料种类:综合考虑\n3.五金材料:装饰拉手、门碰珠、门锁等","m2",4.8,null,null,""]
[4,"实木地板","1、15mm厚实木多层地板","m2",70]
[5,"硅酸钙板窗帘盒","1.窗帘盒材质、规格:12mm夹板+8mm硅酸钙板","m",7.8]
[6,"窗帘","1、阻燃窗帘","m2",24]
[7,"硅酸钙板造型天花","1.龙骨材料种类、规格、中距:U型轻钢龙骨横掌CB60X27中距<1200，U型轻钢次龙骨横掌60X27中距429，10号渡锌抵碳钢丝吊杆，中距横向<800纵向429；钢接混凝土板预留φ10钢筋吊环，中距横向<800，纵向429\n2.面层材料品种、规格:12mm夹板+8mm硅酸钙板","m2",70]
[8,"造型艺术吊灯","1.按建设单位要求定制\n","盏",2]
[9,"天花暗藏LED软灯带",null,"m",120,null,null,"三雄极光、欧普"]
[10,"嵌入式LED筒灯","1、15W","套",40,null,null,"三雄极光、欧普、东莞中工"]
[11,"电气配线","1.名称:电气配线\n2.配线形式:管内穿线\n3.规格:WDZ-BYJ-2.5mm2","m",200,null,null,"南洋电缆、澳通。广缆"]
[12,"电气配线","1.名称:电气配线\n2.配线形式:管内穿线\n3.规格:WDZ-BYJ-4mm2","m",180,null,null,"南洋电缆、澳通。广缆"]
[13,"五孔插座","五孔插座220V、10A","个",20,null,null,"松本电工、施耐德"]
[14,"插座16A",null,"个",4,null,null,"松本电工"]
[15,"开关",null,"个",4,null,null,"松本电工、施耐德"]
[16,"配管 SC25","1.名称:电气配管\n2.材质:镀锌钢管\n3.规格:SC25","m",50]
[17,"网络语音端口","更换原有的网络语音端口","个",10,null,null,"松本电工"]
[18,"分体式变频冷暖空调","1、变频冷暖                                    2、1.5P","台",2,null,null,"美的、格力"]
[19,"冷媒铜管及橡塑保温","1.材质、压力等级:冷媒铜管\n2.规格:Φ9.52\n3.焊接方法:氧乙炔焊\n4.压力试验、吹扫设计要求:空气吹扫\n5.绝热保温:难燃橡塑复合隔热保温套管，20mm","m",30,null,null,"铜管（上海飞轮、华鸿）、橡塑保温（华美）"]
[20,"门禁控制器","指纹、刷卡功能","个",1,null,null,"中控"]
[21,"电磁吸力锁",null,"个",1,null,null,"中控"]
[22,"门磁开关",null,"个",1,null,null,"中控"]
[23,"垃圾清运",null,"项",1]
[24,"拆除原有天花",null,"m2",70]
[25,"拆除原有办公卡座",null,"项",1]
[26,"消防烟感及喷淋改造","新增烟感及喷淋并入园区消防系统","项",1,null,null,"同业主现使用一个品牌"]
["申请人："]